HX711

* Download zip file and remove -master from name and rezip it again (<https://github.com/bogde/HX711> )
* In IDE sketch > include library
* In serial monitor change to 38400 baud